## Dell 3C920 LOM Network Drivers

### Information and Installation Instructions

## 3Com Driver Installation

### Information and Installation Instructions

Revised on 19 February, 2002

Copyright (C) 1998, 1999, 2000, 2001, 2002 Dell Computer Corporation. All rights reserved.
http://www.dell.com

To install the network driver for Microsoft Windows 98 and Windows 98 SE, perform the
following steps:
1. Right click the My Computer icon, and select Properties.

2. Click on Device Manager tab. Select PCI Ethernet Controller and click
on Properties.

3. At the next screen, click the Driver tab, select Update Driver.

4. At next screen, select Next, then select Display a list of all the
drivers in a specific location, so you can select the driver you want.

5. Click Next and at next screen select Have Disk.

6. At Install From Disk screen, select Browse, to find the directory the driver was extracted to c:\Dell\drivers\R39075\Windows\Update\Source. click OK.

7. At Next Screen, click OK again. Files will be copied to your hard drive.

8. When file copy is done, click Finish. You will need to restart the
system for the drivers to be loaded.

To reinstall the network driver for Microsoft Windows Me:
1. Right click the My Computer icon, and select Properties.

2. Click on Device Manager tab.

3. Click on the + (plus) sign next to Network Adapters and highlight 3Com
3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible).

4. Click on Properties tab.

5. Click on Driver tab.

6. Select Update Driver.

7. At next screen, select Specify the location of the driver (Advanced)
and click on Next.

8. At next screen, select Specify a location: and then Browse to find
the directory the driver was extracted to c:\Dell\drivers\39075\Windows\Update\Source.
click OK.

9. Click Next, at the next three screens to begin the file copy process.

10. Click Finish to complete the installation and select Yes when
prompted to restart your computer.

To reinstall the network driver in Microsoft Windows 2000, perform the following steps:
1. Click on Start Menu | Settings | Control Panel | System.

2. Click on the Hardware Tab, and click the Device Manager button.

3. Click on + by Network Adapters.

4. Double click on 3Com 3C920 Integrated Fast Ethernet Controller.

5. Click on Driver tab, and then click on the Update Driver button.

6. At next screen, select Next, then select Display a list of all the
drivers in a specific location, so you can select the driver you want. Click Next.

7. Select Have Disk, and use the Browse button to point to the directory
the driver was extracted to: c:\Dell\drivers\R39075\Windows\Update\Source.

8. Click Open, then OK.

9. At the Select Adapter screen, select 3Com 3C920 Integrated Fast
Ethernet Controller (3C905C-TX Compatible), click Next, then click Next
again.

10. Click Finish to complete the installation.

11. Close the Adapter Properties window.

To reinstall the network driver for Microsoft Windows XP:

1. Click on Start Menu | My Computer | View System Information.

2. Click on the Hardware Tab, and click the Device Manager button.

3. Click on + by Network Adapters.

4. Double click on 3Com 3C920 Integrated Fast Ethernet Controller.

5. Click on Driver tab, and then click on the Update Driver button.

6. Select Install from a list or specific location (advanced), click Next.

7. Select Don't Search. I will choose the driver to install, click Next.

8. Select Have Disk, and use the Browse button to point to the directory
the driver was extracted to. c:\Dell\drivers\R39075\Windows\Update\Source.

9. Click Open, then OK.

10. At the Select Adapter screen, select 3Com 3C920 Integrated Fast
Ethernet Controller (3C905C-TX Compatible), click Next.

11. Click Finish to complete the installation.

12. Close and open windows related to the installation.